3

TABLE D. Connectionless T ransport r equir ed Network Services

TABLE E. TPDU Encoding

TABLE F . Connectionless T ransport Resour ces

Index Description Reference Status N/A Support D.a Connectionless mode network service 6.2 q M D.b N-UNITDA TA.request 6.2.2 q M D.c N-UNITDA TA.indication 6.2.2 q M D.d Connection oriented network service 6.3 q O D.e N-CONNECT .request 6.3.2 q C1 D.f N-CONNECT .indication 6.3.2 q C1 D.g N-CONNECT .response 6.3.2 q C1 D.h N-CONNECT .con�rmation 6.3.2 q C1 D.i N-DA TA.request 6.3.2 q C1 D.j N-DA TA.indication 6.3.2 q C1 D.k N-DISCONNECT .request 6.3.2 q C1 D.l N-DISCONNECT .indication 6.3.2 q C1 D.m N-RESET .indication 6.3.2 q C1 D.n N-RESET .response 6.3.2 q C1

1. Mandatory only if run over Connection Oriented Network

Index Description Reference Status N/A Support E.a Length Indicator 7.1 q M E.b Fixed Part 7.1 q M E.c Variable Part 7.1 q O E.d Data Field 7.1 q O

Index Description Reference Status N/A Support F.a TPDU timer An A.5.1 q M F.b Hold T -UNITDA TA while waiting for net. conn. An A.6.1 q O F.c Allow retention of network connection An A.6.4 q C

2

The following Protocol Implementation Conformance Statement was derived from the document titled �Final text of ISO/DIS 8602: Information processing systems Open System Interconnection - Protocol for providing the connectionless-mode transport service� dated 1987-06-30.

Status Symbols Used M Mandatory O Optional to implement. If implemented the feature may or may not be used. C Conditional. This item becomes mandatory if the related speci�cation or requirement is satis�ed

Support Symbols Used o Indicates that the box should be checked if the implementation contains the item.

TABLE A. Connectionless T ransport TPDU services

TABLE B. Connectionless T ransport Data T ransfer

TABLE C. Connectionless T ransport Data Reception

Index Description Reference Status N/A Support A.a Network service selection 5.3.2.2 o M A.b Address mapping 5.3.2.3 o M

Index Description Reference Status N/A Support B.a TPDU transfer 6.1.3 o M B.b TSDU UNITDA TA Checksum 6.2.3 o O B.c TSDU UNITDA TA Source TSAP-ID 6.2.3 o M B.d TSDU UNITDA TA Destination TSAP-ID 6.2.3 o M B.e TSDU UNITDA TA User Data 6.2.3 o M B.f UN-PROT OCOL IDENTIFIER (PR T-ID) 6.3.3 o O B.g TSDU UNITDA TA quality of service 6.2.4.1 o M

Index Description Reference Status N/A Support C.a TPDU receive 6.2.4.2 o M C.b TSDU UNITDA TA Checksum 6.2.4.2 o O C.c TSAP UNITDA TA source ID 6.2.4.2 q M C.d TSAP UNITDA TA destination ID 6.2.4.2 q M C.e TSAP UNITDA TA user data 6.2.4.2 q M C.f TSAP quality of service 6.2.4.2 q O

1

Lyman:

As I mentioned previously , we have developed a PICS proforma for ISO 8602. The tables for the PICS are enclosed here. If there is national or international interest in such a document, we would like to participate in its development.

Thanks,

Scott Hiles