North America:

Berkeley Software Design, Inc. 3110 Fairview Park Drive, Suite 580 Falls Church, Virginia 22042 USA

Australia and New Zealand:

Berkeley Software Design Int. 1st Floor, 2 King Street Newtown NSW 2042 Australia

Europe:

Berkeley Software Design, Int. Katallin, Town Lane Chartham Hatch, Kent CT4 7NN United Kingdom

Please send to:

Order Form

Ship To: Bill To:

Name

Company

Addr ess

Telephone Fax Electr onic mail

Quantity Description Cost (US $) Total

BSD/386 software on QIC-150 cartridge tape and 60 days support $ 995

BSD/386 software on 5.25” floppies and 60 days support $ 1,245

BSD/386 software on 3.5” floppies and 60 days support $ 1,245

Additional Binary Right To Use licenses $ 200

One year of electronic mail support and upgrades $ 500

One year of telephone support and upgrades $ 1,500

Additional Right To Use support $ 50

Billing Charge (if payment is not enclosed) $ 50

Foreign Shipping and Handling $ 50

Grand Total

Please send me Payment Options

The beta test version of BSD/386 with a free upgrade

to the production version. I acknowledge that beta test software is not suitable for review or production systems.

Charge my Master Card/VISA when shipped.

Account Number Exp. Date Signature

The production system as soon as it is available.

The 60 days support starts on receipt of the production system.

Payment enclosed.

Further information and add me to your mailing list. Bill me ($50 additional).

Supported Hardwar e

Bus Any 386/486 ISA (EISA and MCA coming)

Floating Point Hardwar e Any Intel 387 or compatible (optional)

Disks Any ST 506, RLL, IDE or ESDI

Streaming Tape Contr ollers QIC-02, QIC-36

Displays Mono, EGA, VGA

Mice Logitech, MicroSoft, Mouse Systems

Ethernet boards WD8003, WD8013, Novell NE1000, NE2000, 3com 3C507

SCSI

Contr ollers Disks Tapes

Adaptec 1542b Any SCSI disks Archive 2150S

Serial Ports Includes 16550 FIFO chips

Example Hardwar e Known to W ork

Systems Gateway 2000 486/33 ISA High Definition Systems 486/25 ISA 386 SX/16 ISA ACCELL 486/33 ISA 386/40 ISA

Mother Boards Micronics 486/33, EISA Tech 80386SX 16 MHz, several no-name generics

Contr ollers IDE ESDI

SCSI

CCAT100A, many no-name generics UltraStor Ultra 12F, Data Technology DTG 6282-24, WD1007V-SE2, several no-name generics Adaptec 1542b

Disks IDE ESDI SCSI

Western Digital Miniscribe 380, Maxtor XT-8380E, Maxtor 8800 Maxtor 8380S

Tapes

QIC-02 SCSI

Wangtek 5150PK (QIC-150) Archive 2150S

Ethernet WD Elite 16 Ethercard Plus, WD 8003E, Novell NE2000, 3Com Etherlink 16 (3C507)

Super VGA Cards 1024 x 768 resolution with X

Diamond Speedstar, Orchid ProDesigner II

Recommended System

System 486, or 386 with 387, ISA bus

RAM 4 MB; 8 MB to 12 MB with X

Tape QIC-150 cartridge

Disk Drive 100 MB minimum, 300 MB for active work with sources

Display SVGA board with 1 MB memory and high bandwidth (70 MHz or more). Non-interlaced monitor with high frequency (70 KHz) and high bandwidth (70MHz)

Frequently Asked Questions

Is SCSI supported?

Yes. Support for the Adaptec 1542b controller and disk and tape will be on the beta tape. Additional SCSI controllers will be supported in the production system.

When will the production system be available?

Summer 1992.

What is QIC-150?

QIC-150 is the quarter inch cartridge tape commonly used on workstations. Examples for the ISA Bus include the Wangtek 5150PK or the Archive 2150S.

What displays are supported?

This is a list of cards known to work with X11R5 which we are supplying with the BSD/386 system. This is not an exclusive list, but rather a list of what is known to work. These are currently supported in 256 color mode ONLY and usually require that the card have the maximum memory it is capable of supporting (for 1024x768, 1MB).

What are the licensing terms?

BSD/386 is licensed on a per-system basis. Binary Right To Use licenses are available at $200 each and departmental licenses are available. OEM pricing is also available.

Will binary only versions be available?

Binary distributions will be available in late 1992.

What about binary compatibility?

The production system is planned to support SCO UNIX V.3.3 binaries. This will enable access to a large body of third party packages.

Super VGA Cards MaxResolution Chip Set

Compuadd Hi-Rez card w/1meg 1024x768 ET4000 Diamond SpeedStar 1024x768 ET4000 EIZO MD-10 800x600 ET3000 GENOA 5300/5400 800x600 ET3000 GENOA 6400 800x600 GVGA Optima Mega/1024 1024x768 ET4000 Orchid ProDesigner 800x600 ET3000 Orchid ProDesigner II/1024 1024x768 ET4000 Paradise VGA Professional 640x480 PVGA1A Paradise VGA 1024 640x480 WD90C00 Sigma Legend 1024x768 ET4000 STB PowerGraph w/1meg 1024x768 ET4000 Swan SVGA equipped with VCO chip 1024x768 ET4000 TRICOM Mega/1024 1024x768 ET4000

Supported Mice

Logitech MicroSoft MMSeries Mouse Systems

BSD/386 Source – $995

Source – The only truly open system

North America: Berkeley Softwar e Design, Inc. 3110 Fairview Park Drive Suite 580 Falls Chur ch, Virginia 22042 USA

Toll Free:

+1 800 ITS UNIX

Phone: +1 703 876 5040 Fax: +1 703 876 5059 Email: bsdi-info@bsdi.com

Australia and New Zealand:

Berkeley Software Design Int. 1st Floor, 2 King Street Newtown NSW 2042 Australia

Phone: +61 2 550 5014 Fax: +61 2 519 2551 Email: enquiry@bsdi.oz.au

Europe:

Berkeley Software Design, Int. Katallin, Town Lane Chartham Hatch, Kent CT4 7NN United Kingdom

Phone: +44 227 781 675 Fax: +44 227 762 554 Email: bsdi@hillside.co.uk

BSD – The Other Choice

BSD/386 is a trademark of Berkeley Softwar e Design, Inc.

While some other companies talk about having open systems, Berkeley Software Design, Inc. (BSDI) is proud to be the first and only company to provide the ultimate open system – SOURCE – at a price affordable to end users.

BSD/386 is a “Berkeley UNIX” compatible operating system for the 386 and 486 PC architectures. It is based on the most recent release from the Computer Systems Research Group of the University of California, Berkeley – the Networking Release 2. The NET2 tape contained no AT&T licensed code, but was not a complete system. BSDI has completed the system and added additional drivers. The resulting system does not require a license from AT&T, and so is available in source form at a fraction of AT&T’s price.

BSD/386 is a complete system. There are no optional modules or multiuser fees. The system includes full TCP/IP networking; the X Window System, Version 11, Release 5; POSIX functionality; ANSI C; C++; a reimplementation of Sun’s Network File System (NFS); text processing software (groff, TEX); and more.

BSD/386 comes with 60 days of support and a 90 day money back guarantee.

Alpha distributions are already in the field with beta shipments planned for early February. Beta sites receive free support until the production system ships and a free upgrade to the production system. The standard 60 day support begins with the shipment of the production system.